-=##=oooooo===<
FLUTE by Chris C. N. Chu, Iowa State University
http://class.ee.iastate.edu/cnchu/

FLUTE is freely available for academic use.
Binary and source code distributions of UMpack authorized
for industrial use (not containing FLUTE) are
available unconditionally upon request from the
UMpack maintainers.


Annealer Parameters: 
   normalizing Time:  30000
   start Time:        30000
   cooling Time:      0.01
   fixed-outline?     No
   minimize WL?       Yes
    minimize Steiner WL?  No
    -wireWeight =  0.4
    -areaWeight =  0.4
   scale terminals?        Yes
   soft blks exist?        Yes
   use initial placement?  Yes
   compact init plmt?      No
   compact final plmt?     Yes
   use quad-pl as initial? No

Reading Nodes (files C:\cygwin\tmp\Soc.blocks and C:\cygwin\tmp\Soc.pl)
Reading Nets (file C:\cygwin\tmp\Soc.nets)
Done creating DB 

***** START: round 1 / 1 *****
The random seed for this run is: 1439566684

----- Converting placement to initial solution -----
----- done converting -----

----- Annealing with BTree -----
405.603 micro seconds per move.
NumMoves attempted: 35904
realTime:18.5616	userTime:18.4705
Final Area: 9.84224e+007 WhiteSpace 8.50638% AR 0.685819 HPWL 2.34943e+013
width:  8215.84 
height: 11979.6 
area utilization (wrt. total current area): 92.1605%
whitespace       (wrt. total current area): 7.83952%
----- Annealing with BTree -----

----- Compacting the final solution -----
round[0] 8 blks moved, area: 98422400.00 -> 98160664.00
round[1] 0 blks moved, area: 98160664.00 -> 98160664.00
----- done compacting -----
Original HPWL: 3.44438e+013
bottom HPWL: 3.44438e+013
top HPWL: 3.72385e+013
left HPWL: 3.44438e+013
right HPWL: 4.64709e+013
bottom-left HPWL: 3.44438e+013
bottom-right HPWL: 4.64709e+013
top-left HPWL: 3.72978e+013
top-right HPWL: 4.23306e+013
left-bottom HPWL: 3.44438e+013
right-bottom HPWL: 4.64709e+013
left-top HPWL: 3.72385e+013
right-top HPWL: 5.01702e+013
minimum HPWL: 3.44438e+013 in the original position.
packing design towards the original position
final HPWL: 3.44438e+013
OutPut Plot file is out.plt
Saving C:\cygwin\tmp\meshsoc.pl as output .pl file
***** DONE:  round 1 / 1 *****

***** SUMMARY of all rounds *****
         Area: Min: 9.81607e+007 Average: 9.81607e+007 Max: 9.81607e+007
         HPWL: Min: 3.44438e+013 Average: 3.44438e+013 Max: 3.44438e+013
Unweighted HPWL: Min: 50339.5 Average: 50339.5 Max: 50339.5
   WhiteSpace: Min: 8.21782% Average: 8.21782% Max: 8.21782%
Average Time: 18.5641
